DESD Lab 6: Assembler

1 Background

Low-level machine programs are rarely written by humans. Typically, they are generated by compilers. Yet humans can inspect the translated code and learn important lessons about how to write their high-level programs better, in a way that avoids low-level pitfalls and exploits the underlying hardware better.

One of the key players in this translation process is the assembler {a program designed to translate code written in a symbolic machine language into code written in binary machine language.

This project marks an exciting landmark in our Nand to Tetris odyssey: it deals with building the first rung up the software hierarchy, which will eventually end up in the construction of a compiler for a Java-like high-level language. But, first things first.

2 Objective

Write an Assembler program in Matlab that translates programs written in the symbolic Hack assembly language into binary code that can execute on the Hack hardware platform built in the previous projects.

3 Contract

There are three ways to describe the desired behavior of your assembler:

1. When loaded into your assembler, a Prog.asm file containing a valid Hack assembly language program should be translated into the correct Hack binary code and stored in a Prog.hack file.
2. The output produced by your assembler must be identical to the output produced by the Assembler supplied with the Nand2Tetris Software Suite.
3. Your assembler must implement the translation specification given in Chapter 6, Section 2.

4 Usage

The Matlab assemble program should be invoked using something like "Assembler fileName.asm", where the string fileName.asm is the assembler's input, i.e. the name of a text file containing Hack assembly commands. The assembler creates an output text file named fileName.hack. Each line in the output file consists of sixteen 0 and 1 characters. The output file is stored in the same directory of the input file. The name of the input file may contain a file path.

5 Resources

The relevant reading for this project is Chapter 6. Your assembler implementation should be written in Matlab programming language. Two useful tools are the supplied Assembler and the supplied CPU Emulator, both available in your tools directory. These tools allow experimenting with a working assembler before setting out to build one yourself. In addition, the supplied assembler provides a visual line-level translation GUI, and allows code comparisons with the outputs that your assembler will generate. For more information about these capabilities, refer to the supplied Assembler Tutorial (PPT, PDF)

6 Proposed Implementation

Chapter 6 includes a proposed, language-independent Assembler API, which can serve as your implementation's blueprint. We suggest building the assembler in two stages. First, write a basic assembler designed to translate assembly programs that contain no symbols. Next, extend your basic assembler with symbol handling capabilities, yielding the final assembler. The test programs that we supply below are designed to support this staged implementation strategy.

7 Test Programs

Each test program except the first one comes in two versions: Prog.asm is an assembly program; ProgL.asm is the very same program, less the symbols (each symbol is replaced with an explicit memory address).

8 Tools

The supplied Hack Assembler shown below is guaranteed to generate correct binary code. This guaranteed performance can be used to test if another assembler, say the one written by you, also generates correct code. The following screen shot illustrates the comparison process:



The comparison logic: Let Prog.asm be some program written in the symbolic Hack assembly language. Suppose we translate this program using the supplied assembler, producing a binary file called Prog.hack. Next, we use another assembler (e.g. the one that you wrote) to translate the same program into another file, say MyProg.hack. Now, if the latter assembler is working correctly, it follows that Prog.hack == MyProg.hack. Thus, one way to test a newly written assembler is as follows:

(i) Load into the supplied visual assembler Prog.asm as a source program and MyProg.hack as a compare file, (ii) translate the source program, and (iii) compare the resulting binary code with the compare \_le (see the \_gure above). If the comparison fails, the assembler that generated MyProg.hack must be buggy; otherwise, it may be OK.

9 Report

The report document should not exceed 3000 ±10% words. The style guide, provided at the end of this lab sheet, should be used. The following outline can be used to structure the text:

* Abstract

What did you do?

How did you do it?

What did you learn?

* Need definition

Why do we need an assembler?